
# **napari-LF plugin For viewing and processing light field images with the napari viewer**

# **User Guide**



The above screenshot shows an interactive napari viewer with a light field image of a fluorescently labeled giant unilamellar vesicle (GUV). On the right side is the widget for the napari-LF plugin that can be used to view, manipulate, and process light field images.

napari-LF builds on existing python code for processing light field images, typically recorded on a microscope. The code, called LFAnalyze, was developed by Michael Broxton in the laboratory of Marc Levoy at Stanford University between 2010 and 2013 (Broxton et al., 2013). The code includes an iterative deconvolution routine for light field images of fluorescently labeled, transparent specimens or similar objects whose optical properties are characterized by a single parameter associated with voxels in object space (e.g. fluorescence density or absorption coefficient).

The Github repository for napari-LF is:

<https://github.com/PolarizedLightFieldMicroscopy/napari-LF.git>

Reference:  
Broxton, M., Grosenick, L., Yang, S., Cohen, N., Andalman, A., Deisseroth, K. and Levoy, M. (2013). Wave optics theory and 3-D deconvolution for the light field microscope. Optics Express, 21(21):25418-25439. https://doi.org/10.1364/OE.21.025418

The following is copied from the current (July 2022) README.md file of the Github repository:

napari-LF provides three basic processes to Calibrate, Rectify, and Deconvolve light field images:

The **Calibrate** process generates a calibration file that represents the optical setup that was used to record the light field images. The same calibration file can be used to rectify and deconvolve all light field images that were recorded with the same optical setup, usually the same microscope and light field camera. The Calibrate process requires as input the radiometry frame, dark frame, optical parameters, and volume parameters to generate the calibration file, which is subsequently used to rectify and deconvolve related light field images. The calibration file includes a point spread function (PSF) derived from the optical and volume parameters and is stored in HDF5 file format.

The **Rectify** process uses the calibration file for an affine transformation to scale and rotate experimental light field images that were recorded with a light field camera whose microlens array was (slightly) rotated with respect to the pixel array of the area detector and whose pixel pitch is not commensurate with the microlens pitch. After rectification, the rectified light field has the same integer number of pixels behind each microlens. When the Deconvolve process is called for an experimental light field image, rectifying the light field image is automatically applied before the iterative deconvolution does begin. However, the rectified light field image is not saved and is not available for viewing. Therefore, by pushing the Rectify button in the middle of the napari-LF widget, only the rectification step is invoked and the rectified light field image is saved to the project directory.

The **Deconvolve** process uses the PSF and a wave optics model to iteratively deconvolve a light field image into a stack of optical sections.

The **Parameter** panels, located in the lower half of the napari-LF widget, allows the user to specify settings for the reconstruction process. Once the appropriate parameters are selected, the Calibrate button followed by the Deconvolve button can be pushed to complete the reconstruction.

# Quickstart

1. Install the napari-LF plugin into your napari environment, as described below under **Installation**.
2. From the napari Plugins menu, select the napari-LF plugin to install its widget into the napari viewer
3. Near the top of the widget, select your image folder containing the following images: light field, radiometry, and dark frame.
4. Write the name of the metadata file you want for recording your reconstruction settings, e.g. metadata.txt. This file will be updated each time a calibration process is started
5. Calibration

* In the parameters panel, navigate to **Calibrate**, **Required** (top tab **Calibrate**, bottom tab **Required**), which is the default selection.
* Select **radiometry** and **dark frame** images from pull down menus.
* Write the name of the **calibration file** you would like to produce, e.g. calibration.lfc.
* Enter the appropriate **optical parameters** according to your microscope and sample material.
* Enter the v**olume parameters** you would like for your 3D reconstruction.
* Push the **Calibrate button**.

1. Deconvolution

* In the parameters panel, navigate to **Deconvolve, Required**.
* Select **light field**image and **calibration file** from pull down menus.
* Write the name of the **output image stack** you would like to produce, e.g. output\_stack.tif.
* Push the **Deconvolve button**. 3D focal stack reconstruction will display in the napari viewer and be saved in your project image folder.

# Getting Help

For details about each parameter, hover over each parameter textbox to read the tooltip description. For additional information about the reconstruction process, see our documentation on [GitHub](https://github.com/PolarizedLightFieldMicroscopy/napari-LF).

# Installation

Create a virtual environment from the command line for napari with the python libraries necessary for the light field plugin.

conda create --name napari-lf python==3.9 h5py pyopencl napari git -c conda-forge

conda activate napari-lf

Then, install the light field plugin. Below are two methods of installing:

**Method 1:** Install the latest development version from the command line.

pip install git+https://github.com/PolarizedLightFieldMicroscopy/napari-LF.git

**Method 2:** Install a downloaded version.

1. Open napari from the command line.

napari

1. From the menu, select **Plugins > Install/uninstall Packages**.
2. Drag and drop the downloaded **napari-LF** directory into the bottom bar.
3. Select **Install** to install the light field plugin.
4. Close napari.

Lastly, to access the plugin, open napari from the command line.


From the **Plugins menu**, select  **napari-LF LFAnalyze**.

At a future time, you can install napari-LF via [pip](https://pypi.org/project/pip/):

pip install napari-LF

The following pages provide screenshots of the various panels of the widget and comment on the data files, parameters, and functions than can be invoked.

## **Overview of Widget GUI**



**Choose directory**, which contains related images and their processed data. All pull-down menus in the widget will populate with file names from this directory.

**Calibrate, Rectify, Deconvolve panels** are used to display, change, and enter parameters used for data processing. The parameters are explained in more detail on the following pages of this guide.

**Status bar** is green when no process is active, status bar is orange when a process is in progress.

**Calibrate, Rectify, Deconvolve buttons** initiates data processing using parameters defined in related panels below.

**Comments** saved in the metadata.txt file

**Presets drop down menu** populated with globally saved processing parameters

**Metadata file** holds parameters in Calibrate etc., updated when generating new processed data.

Select **images in drop-down menu** and **Open Image** in the viewer

## **Calibrate Required panel**

The Calibrate panel defines the required and optional parameters used to generate the calibration file. The calibration file characterizes the microscope setup and includes the instruments point spread function that is used for deconvolving a light field image recorded with the setup. In addition, the calibration file is specific to the number of z-Slices specified as a parameter, their distance in µm, and the Supersample number. The Supersample number is an integer that specifies the smallest voxel size used for the deconvolution. The smallest voxel size is equal to the microlens pitch divided by the objective lens magnification and by the Supersample integer. Note, however, that the actual deconvolved voxel size is also a function of its distance from the nominal focal plane. The calibration file has the extension .lfc and the HDF5 file format.

Choose from drop-down menus to select

**Radiometry image**: Specify a radiometry frame to use for radiometric correction. If no frame is specified, then no radiometric correction is carried out.

**Dark frame image**: Specify a dark frame image to subtract from the input light-field before processing (This makes radiometric calibration more accurate).

Graphical user interface

Description automatically generated

**Optical parameters** relate to the optical setup used, including the microlens array in front of the area detector, and the microscope objective lens.

Enter **Calibration file** name. When a file with this name already exists, the field is outlined yellow and the Calibrate button has a green check mark. A new calibration will override the file.

Graphical user interface

Description automatically generated

The **Volume parameters** specify the number of z-Slices, their distance in micrometer (um) and the Supersample used. Supersample results in a higher resolution reconstruction up to a point, and interpolation after that point.

More **Optical parameters**, including the tube lens of the microscope, center wavelength of the light recorded, and the refractive index of the medium embedding the sample structure.

## **Calibrate Optional panel**

**Calibration routine parameters**

**Synthetic LF**: Use this option to create a synthetic light field, i.e. with no calibration image

**Use ray optics**: Use the less accurate ray optics model, rather than wave optics model

**Use voxels as points**: Treat voxels as ideal points. This turns off numerical integration that gives the voxel spatial extent (which can be important for anti-aliasing.

**Align radiometry**: Align the radiometry image to the geometric calibration image. Use this option when the radiometry frame was "bumped" before imaging begins.

A screenshot of a computer

Description automatically generated with medium confidence

Additional **Optical** and **Volume parameters**

Graphical user interface, application

Description automatically generated

**Geometric calibration options**

**Affine alignment**: Use affine warp for correcting geometric distortion (default is cubic).

**Isometry alignment**: Use isometry warp for correcting geometric distortion (default is cubic).

**Chief ray image**: Use this flag to indicate that the calibration frame is a chief ray image.

**Other Options**

**Crop center lenslets**: For severe aperture vignetting (high NA objectives), use only center lenslets for calibration, and extrapolate outwards.

**Skip alignment**: Skip the alignment step during geometric calibration. Useful if you are working with an already-rectified light field or a synthetic light field.

**Skip subpixel alignment**: Skip subpixel alignment for determining lenslet centers.

**Number of CPU threads**: Set the number of CPU threads to use when generating the raydb.

**Pinhole filename**: After calibrating, save the rectified light field as a rectified sub-aperture image.

**Lenslet filename**: After calibrating, save the rectified light field as a rectified lenslet image.

A screenshot of a computer

Description automatically generated with medium confidence

## **Calibrate Inspect panel**

The Calibrate Inspect panel prints attributes of the Calibration File selected and the Datasets and Groups of its HDF5 file format

Graphical user interface, text, application

Description automatically generated

**Inspector**

Select **Calibration file** to inspect.

Printed attributes of the HDF5 file format.

Graphical user interface, text, application

Description automatically generated

Printed attributes of the HDF5 file format.

## **Rectify Required and Optional panels**

The calibration file includes instructions for rectifying a light field that was recorded with the microscope setup represented in the calibration file. A rectified light field contains the same information as the original light field, but on a grid which puts an integer number of pixels behind each microlens and generates a light field with an integer number of microlenses in the horizontal and vertical direction. Every deconvolution requires a rectified light field and therefore, rectification is an integral step in the deconvolution process implemented in napari-LF. In addition, the Rectify panel lets one save the rectified light field as an image file for visual inspection.

Graphical user interface, application

Description automatically generated

**Files:**

Choose the original **Light field image** and the **Calibration file** to be used for generating the rectified light field that will be saved using the file name entered under **Rectified image**.

Graphical user interface, application

Description automatically generated

**Misc**

**Subaperture**: Save out the light field image as tiled subapertures or pinhole views.

**Output pixels per lenslet**: Specify the number of pixels per lenslet in the output image.

## **Deconvolve Required panel**

Graphical user interface, application

Description automatically generated

**Files**

From the drop-down menus, choose the **Light field image** and the **Calibration file** to be used for generating the deconvolved stack that will be saved using the file name entered under **Output image stack**.

**Algorithm selection**

Available reconstruction methods are:

**amp**: Approximate Message Passing with optional multiscale denoising**.**

**admm\_huber**: Alternating Direction Method of Multipliers with Huber loss**.**

**admm\_tv**: Alternating Direction Method of Multipliers with TV penalty.

**cg**: Conjugate Gradient.

**direct**: Direct method with Cholesky factorization.

**lsqr**: Least Squares QR.

**kspace**: k-space deconvolution.

**sirt**: Simultaneous Iterative Reconstruction Technique.

**mrnsd**: MRNSDand

**rl**: Richardson-Lucy.

Default is currently **rl**.

**Alpha**: Relaxation parameter for SIRT-based iterative reconstruction.

**Multiscale smoothing**: Multiscale regularization option for AMP reconstruction.

**Save multiscale**: Save multilevel decomposition of data.

## Deconvolve Optional panel

Graphical user interface, application

Description automatically generated

## **Deconvolve Optional panel**

**Generic parameters for iterative reconstruction routines**

**Regularization lambda**: Regul. coefficient whose behavior varies by reconstruction algorithm.

**Regularization lambda2**: Additional coefficient. Behavior varies by algorithm, and not all algorithms use two regularization coefficients.

**Max iterations**: Maximum number of iterations for SIRT-based reconstruction.

**Convergence threshold**: Convergence criteria threshold, d/dt (MSE). Try 5e-5 for SIRT, 1e-2 for TV.


Graphical user interface

Description automatically generated

**Noise model parameters**

**Read noise variance**: Set the variance of the measured camera read noise.

**Background level**: Set the measured background level of the image.



**Assorted other parameters**

**Focal stack**: Turn off deconvolution and simply save a focal stack to disk.

**Remove grid**: Remove grid artifacts in light field image using spectral median filter.

**Pinhole filename**: After deconvolution, save out a deconvolved light field sub-aperture image.

**Deconvolution type**: Choose deconvolution method, one of algebraic, direct, admm

**Registration factor**: Regularization parameter used in ADMM.

**HDF5 covariance filename**: Specify filename

**Log convergence**: For logging convergence details

## **Hardware panel**

Graphical user interface, application

Description automatically generated

**Select device**: Force Ifdeconvolve to use a specific GPU on your system. If not supplied, this will default to $USE\_GPU\_ID or 0; if --gpu-id is not supplied, it will default to the value of the USE\_GPU\_ID environment variable, if set, or 0 otherwise

**Select Platform**: Force Ifdeconvolve to use a specific OpenCL Platform on your system.

**Use single precision**: Use single precision float instead of double.

**Disable GPU**: Disable GPU deconvolution and use software implementation instead.

## **Miscellaneous panel**

Graphical user interface, application

Description automatically generated

**Use system/external viewers**: Use system/external viewer for displaying images instead.

**System viewer**: Chose your viewer, either System: OS default, or External: User selects path under **External viewer**.

**Disable mousewheel on combobox and spinner widgets:** Disable mousewheel on combobox and spinner widgets to avoid accidentally changing values.